CHANNEL HOOKUP

Address(Dim) Ch Position Unit Type, Accessories, Watts Purpose Color & Template

5 1 House Electric 26” Source Four 750W A 05/119 & 51/119

7,48 2 House Electric 26” Source Four 750W B 05/119 & 51/119

3, 6 3 House Electric 26” Source Four 750W C 05/119 & 51/119

2, 45 4 House Electric 26” Source Four 750W D 05/119 & 51/119

1 5 House Electric 26” Source Four 750W E 05/119 & 51/119

10, 20 6 1st Electric 6” Fresnel/Barn Door/ 500W F 05/119 & 51/119

14, 17 7 1st Electric 6” Fresnel/Barn Door/ 500W G 05/119 & 51/119

13, 18 8 1st Electric 6” Fresnel/Barn Door/ 500W H 05/119 & 51/119

11, 19 9 1st Electric 6” Fresnel/Barn Door/ 500W I 05/119 & 51/119

22, 32 10 2nd Electric 6” Fresnel/Barn Door/ 500W J 05/119 & 51/119

26 11 2nd Electric 6” Fresnel/Barn Door/ 500W K 05/119 & 51/119

29 12 2nd Electric 6” Fresnel/Barn Door/ 500W L 05/119 & 51/119

21, 31 13 2nd Electric 6” Fresnel/Barn Door/ 500W M 05/119 & 51/119

37 14 US Baton Vivid-R 11 LED F-A-B

42 15 US Baton Vivid-R 11 LED G-B-C

41 16 US Baton Vivid-R 11 LED H-D-C

38 17 US Baton Vivid-R 11 LED I-D-E

18 1st Electric Vivid-R 11 LED B-C

19 1st Electric Vivid-R 11 LED D-C

-- 20 Open Special

-- 21 Open Special

-- 22 Open Special

-- 23 Open Special

-- 24 Open Special

8,56,4 SP House Electric 26” Source Four 750W SP

9,15, SP 1st Electric 26” Source Four 750W SP

23 50 2nd Electric 50” Source Four 750W Gobo Breakup